For 1990-2009 cars

### Removal Procedure

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.
2. Remove the right sound insulator. Refer to Instrument Panel Insulator Panel Replacement - Right Side in Instrument Panel, Gauges and Console.
3. Remove the instrument panel (IP) compartment. Refer to Instrument Panel Storage Compartment Replacement in Instrument Panel, Gauges and Console.
4. Disconnect the electrical connectors from the programmer.
5. Remove the retaining tabs from the programmer.
6. Remove the programmer.

### Installation Procedure

Important: After replacing the programmer, recalibrate the actuators for proper travel. Cycle the ignition ON for 3 minutes in order to allow the programmer and the actuator to recalibrate for proper travel.

1. Install the programmer into the retainer on the bracket.
2. Connect the electrical connectors to the programmer.
3. Install the instrument panel (IP) compartment. Refer to Instrument Panel Storage Compartment Replacement in Instrument Panel, Gauges and Console.
4. Install the right sound insulator. Refer to Instrument Panel Insulator Panel Replacement - Right Side in Instrument Panel, Gauges and Console.
5. Connect the negative battery cable.
6. Recalibrate the actuators.