For 1990-2009 cars

### Removal Procedure

1. Lower the formed headliner at the rear. Refer to Headlining Trim Panel Replacement in Interior Trim.
2. Remove the express module (2) by sliding the module out of the slots in the bracket (toward the center of the vehicle).
3. Disconnect the wiring connector to the express module.

### Installation Procedure

1. Connect the wiring connector to the express module (2).
2. Install the express module (2).
3. Secure the formed headliner. Refer to Headlining Trim Panel Replacement in Interior Trim.
4. Inspect sunroof for proper operation.