For 1990-2009 cars

### Removal Procedure

#### Tool Required

J 42562 Snap Ring Tool

1. Remove the case extension housing. Refer to Case Extension Replacement .
2. Disconnect the left drive axle from the transaxle. Refer to Wheel Drive Shaft Replacement in Drive Axle.
3. Rotate the differential carrier until the end of the output shaft can be seen and the differential pinion shaft (701) is in a horizontal position.
4. Place the J 42562 between the end of the output shaft and the differential pinion shaft.
5. Using a hammer, hit the end of the axle removal tool in order to compress the output shaft compression ring (512) and push the output shaft through the differential side gear.
6. Remove the differential carrier (700).
7. Using snap ring pliers remove the compression ring (512) from the output shaft.

Important: Be careful not to damage the bearing (511) on the output shaft.

8. Remove the output shaft through the left wheel opening.
9. Inspect the output shaft (510) and the bearing (511) for the following:

• | A cracked or deformed bearing cage

• | Damaged bushing journals

• | Stripped splines

• | A damaged retainer ring groove

### Installation Procedure

1. Install the drive axle retaining ring (509) and the output shaft differential inboard snap ring (512) onto the output shaft (510).
2. Install the fourth clutch bearing (511) onto the output shaft (510).
3. Hold the front differential carrier (700) in place and carefully install the output shaft (510) into the transmission through the left wheel opening. Extend the output shaft through the differential side gear.
4. Install the case extension housing. Refer to Case Extension Replacement .
5. Connect the left drive axle to the transaxle. Refer to Wheel Drive Shaft Replacement in Drive Axle.