For 1990-2009 cars

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---
1 | Press the rear compartment lid release button on the keyless entry transmitter. | The rear compartment lid opens. |

• | Rear Compartment Lid Release Inoperative

• | Rear Compartment Lid Release Inoperative

2 |

1. Insert the ignition key into the rear compartment lid release switch (mounted on the IP) and turn it to the unlock position.
2. Press the rear compartment lid release switch mounted on the IP.

The rear compartment lid opens.

• | Rear Compartment Lid Release Inoperative

• | Rear Compartment Lid Release Inoperative

3 | Use the keyless entry transmitter in order to inspect the following functions:

• | The door lock function

• | The door unlock function

• | The panic alarm function

The doors perform the following functions on command:

• | Lock

• | Unlock

• | Panic alarm

One or more of the keyless entry transmitter functions do not operate. Refer to Remote Keyless Entry System Check in Keyless Entry

* Refer to the appropriate symptom diagnostic table for the applicable abnormal result.