For 1990-2009 cars

# POOR DRIVEABILITY/PERFORMANCE INCORRECT GAS/DIESEL CAMSHAFT

ROLLER LIFT CAMSHAFTS V-8 - DIESEL AND GASOLINE ENGINES

#### MODELS AFFECTED: 1981 - 1985 REGAL, LESABRE AND RIVIERA --------------- 1981 - 1984 ELECTRA

Roller lifter camshafts for 1981-85 V-8 diesel, and 1985 and later V-8 gasoline engines are almost identical, except for lobe contour and their fit to the camshaft adapter. Until recently, it was impossible to inadvertently install the wrong camshaft in an engine because:

- The adapter on a diesel engine is smaller and will not fit a gas camshaft.

- The adapter on a gas engine contains a pin that must fit into a hole. This hole is not drilled on a diesel camshaft.

Shortly, this pin will be removed from the gas adapter. It would then be possible to inadvertently install a diesel camshaft in a gas engine. This will result in poor performance and economy due to cam lobe contour differences.

#### Identification:

--------------

There is .015" difference between the adapter hole size. A gasoline adapter on a diesel camshaft will have a very sloppy fit. The diameter of the camshaft where it fits to the adapter is:

Gasoline - .951 - .952

Diesel - .936 - .937

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.