For 1990-2009 cars

## Rocker Panel Molding Replacement Oldsmobile

### Removal Procedure

1. Remove the screw (3) from the front wheelhouse area.
2. Remove the screws (2) at the lower edge of the rocker panel molding (1).
3. Pull upward on the top edge of the rocker panel molding in order to separate the rocker panel molding from the door sill.
4. Pull outward in order to release the push in retainers.
5. Remove the molding from the body.
6. Remove the damaged retainers from the following components:

• | The body

• | The rocker panel molding (1)

### Installation Procedure

1. Install the new retainers.
2. Position the molding (1) to the vehicle.
3. Press the top edge of the molding onto the door sill.
4. Press the molding in order to engage the retainers.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

5. Install the screws (2) along the lower edge of the molding (1).

Tighten
Tighten the screws to 1.7 N·m (15 lb in).

6. Install the screw (3) to the front wheelhouse area.

Tighten
Tighten the screws to 1.5 N·m (13 lb in).

## Rocker Panel Molding Replacement Buick

### Removal Procedure

1. Remove the screws (2) retaining the wheel opening molding (1).
2. Remove the wheel opening molding (1).

### Installation Procedure

1. Install the wheel opening molding (1).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the screws (2) in order to retain the wheel opening molding.

Tighten
Tighten the screws to 1.6 N·m (14 lb in).