For 1990-2009 cars

### Removal Procedure

1. Remove the right side sound insulator. Refer to Instrument Panel Insulator Panel Replacement - Right Side in Instrument Panel, Guages and Console.
2. Disconnect the electrical connector from the blower motor.
3. Remove the cooling tube from the blower motor.
4. Remove the screws that attach the blower motor to the heater and A/C module assembly.
5. Remove the blower motor and the fan.

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the blower motor to the heater and A/C module assembly using the attaching screws.

Tighten
Tighten the bolt to 1.4 N·m (12 lb in).

2. Install the cooling tube to the blower motor.
3. Connect the electrical connector to the blower motor.
4. Install the right side sound insulator. Refer to Instrument Panel Insulator Panel Replacement - Right Side in Instrument Panel, Guages and Console.