For 1990-2009 cars

# DIM GEAR INDICATOR LIGHT OR REPEAT FAILURE (INCORRECT P/N)

#### MODELS AFFECTED: 1986-1988 RIVIERAS

On Some 1986-88 Rivieras the gear indicator light assembly, after an initial repair, may either appear dim or fail repeatedly.

These conditions may be caused by incorrect service parts use. The 1987-88 electroluminescent inverter is not compatible with the 1986 gear indicator light assembly. This incorrect parts combination may cause indicator light dimness. Also, the 1986 inverter is not compatible with the 1987-88 gear indicator light assembly. This incorrpect parts combination may cause indicator light assembly failure.

To repair either of these conditions, use the appropriate replacement part numbers listed below:

1986 1987-88 ---- ------- Gear Indicator Light Assembly 1639847 1647027 Electroluminescent Inverter 1636499 1642274

#### WARRANTY INFORMATION

Labor Operation: K5100 (Gear Indicator Light Assembly Replacement) Labor Time: 0.3 Hour

Labor Operation: N1690 (Electroluminescent Inverter Replacement) Labor Time: 0.3 Hour Trouble Code: 92

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.