For 1990-2009 cars

#### Range Reference (4T65-E)

| Park | Reverse | Neutral | D | 3 | 2 | 1
--- | --- | --- | --- | --- | --- | --- | ---
Gear |  |  |  | 1st | 2nd | 3rd | 4th | 1st | 2nd | 3rd | 1st | 2nd | 1st
1-2, 3-4 Shift Solenoid | ON | ON | ON | ON | OFF | OFF | ON | ON | OFF | OFF | ON | OFF | ON
2-3 Shift Solenoid | ON | ON | ON | ON | ON | OFF | OFF | ON | ON | OFF | ON | ON | ON
Fourth Clutch | -- | -- | -- | -- | -- | -- | A | -- | -- | -- | -- | -- | --
Reverse Band | -- | A | -- | -- | -- | -- | -- | -- | -- | -- | -- | -- | --
Second Clutch | -- | -- | -- | -- | A | A | A | -- | A | A | -- | A | --
Third Clutch | -- | -- | -- | -- | -- | A | A* | -- | -- | A | -- | -- | A
Third Sprag | -- | -- | -- | -- | -- | H | O | -- | -- | H | -- | -- | H
Input Clutch | A* | A | A* | A | A* | -- | -- | A | A* | A | A | A* | A
Input Sprag | H* | H | H | H | O | -- | -- | H | O | H | H | O | H
2-1 Manual Band | -- | -- | -- | -- | -- | -- | -- | -- | -- | -- | A | A | A
1-2 Support Roller Clutch | -- | -- | -- | H | H | O | O | H | H | O | H | H | H
Forward Band | -- | -- | -- | A | A | A* | A* | A | A | A* | A | A | A

- ON = the solenoid valve is energized.
- OFF = the solenoid valve is de-energized.
- A = Applied
- H = Holding
- O = Overrun
- * = applied, or holding, with no load (not transmitting torque).