For 1990-2009 cars

# SMU - SECTION 6D1 - REVISED BATTERY REPLACEMENT

#### SUBJECT: SERVICE MANUAL UPDATE - SECTION 6D1 - REVISED BATTERY REPLACEMENT PROCEDURE

#### MODELS: 1995-96 BUICK RIVIERA 1995-96 OLDSMOBILE AURORA

THIS BULLETIN IS TO REVISE THE BATTERY REPLACEMENT PROCEDURE ON PAGE 6D1-7 OF THE 1995 AND 6D1-9 OF THE 1996 SERVICE MANUAL. THE PROCEDURE SHOULD READ AS FOLLOWS:

REMOVE OR DISCONNECT:

1. REAR SEAT CUSHION.

2. NEGATIVE BATTERY CABLE.

3. POSITIVE BATTERY CABLE.

4. BOLT AND RETAINER.

5. VENT TUBE.

6. BATTERY.

INSTALL OR CONNECT:

1. BATTERY.

2. VENT TUBE.

3. RETAINER AND RETAINER BOLT.

4. POSITIVE CABLE.

5. NEGATIVE CABLE.

6. REAR SEAT CUSHION.

FIGURES: 00 ATTACHMENTS: 00

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1995 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.