For 1990-2009 cars

#### Tools Required

J 35777 Caliper Piston Seal Installer

1. Remove the caliper from vehicle. Refer to Front Brake Caliper Replacement or Rear Brake Caliper Replacement .

Caution: Do not place your fingers in front of the piston in order to catch or protect the piston while applying compressed air. This could result in serious injury.

2. Remove the piston by directing low pressure compressed air into the caliper inlet hole.

Important: Care must be used when removing the piston boot and seal from the caliper. Use a small plastic or wood tool for removal. Do not use a metal tool because it may damage the caliper bore or seal groove.

3. Remove the piston boot (2) from the caliper (1).
4. Remove the piston seal from the caliper (1).
5. Remove the bleeder valve (5) and cap from the caliper.
6. Clean all of the parts. Use clean, denatured alcohol. Dry all of the parts with unlubricated, low pressure compressed air. Blow out all of the passages in the caliper body and the bleeder valve.
7. Inspect all of the parts as follows.

• | Piston - Inspect for scoring, nicks, cracks, wear, or corrosion. Replace the piston if any damage is found.

• | Caliper Bore - Inspect for scoring, nicks, cracks, wear, or corrosion. Use crocus cloth to polish out light corrosion. Otherwise, replace the caliper. Do not hone the caliper bore.

• | Seal groove in the caliper bore for nicks or burrs. If found, replace the caliper.

8. Install the bleeder valve cap and bleeder valve into the caliper.
9. Install the new piston seal. Lubricate the seal with clean brake fluid before installing.
10. Install the new piston boot over the piston and install the piston into the bottom of the caliper bore. Seat the piston boot using J 35777 boot installer.
11. Install the caliper onto the vehicle. Refer to Front Brake Caliper Replacement or Rear Brake Caliper Replacement .