For 1990-2009 cars

## Driver or Passenger Seat Back Cushion Cover and Pad Replacement Buick

### Removal Procedure

1. Remove the seat. Refer to Seat Replacement .
2. Remove the seat back. Refer to Front Seat Back Replacement .
3. Remove the head restraint. Refer to Front Seat Head Restraint Replacement .
4. Disconnect the fasteners to the seat back hinge assembly.
5. Remove the seat back (3).
6. Disengage the retainer (1) at the bottom of the seat back cover.
7. Disengage the fasteners from the seat back cover as the cover is being lifted.
8. Separate the seat back cover from the cushion.
9. Disengage the head restraint guides (1).
10. Remove the cover (3) and the cushion (4).

### Installation Procedure

1. Install the cushion (4) onto the seat back frame (5).
2. Install the seat back cover (3).
3. Install the seat back cover fasteners.
4. Engage the head restraint guides (1).
5. Install the head restraint (2). Refer to Front Seat Head Restraint Replacement .
6. Engage the retainer (1) at the bottom of the seat back cover.
7. Connect the fasteners to the seat back (5) hinge assembly.
8. Install the seat back. Refer to Front Seat Back Replacement .
9. Install the seat. Refer to Seat Replacement .

## Driver or Passenger Seat Back Cushion Cover and Pad Replacement Oldsmobile

### Removal Procedure

1. Remove the seat. Refer to Seat Replacement .
2. Remove the seat back. Refer to Front Seat Back Replacement .
3. Remove the head restraint. Refer to Front Seat Head Restraint Replacement .
4. Remove the seat back cover to the position of the head restraint (2).
5. Remove the head restraint guides (1). Refer to Front Seat Head Restraint Replacement .
6. Remove the seat back cover (3).
7. Separate the seat back frame (5) from the cushion (4).
8. Remove the cushion (4).

### Installation Procedure

1. Install the cushion (4).
2. Install the seat back frame (5) to the cushion (4).
3. Install the seat back cover (3).
4. Install the head restraint guides (1). Refer to Front Seat Head Restraint Replacement .
5. Install the seat back cover to the position of the head restraint (2).
6. Install the head restraint. Refer to Front Seat Head Restraint Replacement .
7. Install the seat back. Refer to Front Seat Back Replacement .
8. Install the seat. Refer to Seat Replacement .