For 1990-2009 cars

DTC/Description | Type | Illuminate AIR BAG Warning Indicator
--- | --- | ---
DTC B1015 Passenger Deploy. Loop Resistance High | SDM | Yes
DTC B1016 Passenger Deployment Loop Resistance Low | SDM | Yes
DTC B1017 Passenger Deployment Loop Open | SDM | Yes
DTC B1018 Passenger Deployment Loop Short to GND | SDM | Yes
DTC B1019 Passenger Deploy. Loop Short to Voltage | SDM | Yes
DTC B1021 Driver Deployment Loop Resistance High | SDM | Yes
DTC B1022 Driver Deployment Loop Resistance Low | SDM | Yes
DTC B1024 Driver Deployment Loop Short to Ground | SDM | Yes
DTC B1025 Driver Deployment Loop Short to Voltage | SDM | Yes
DTC B1026 Driver Deployment Loop Open | SDM | Yes
DTC B1035 Discr. Sensor Closed or Short to GND | SDM | Yes
DTC B1036 Discr. Sensor Open or Short to Voltage | SDM | Yes
DTC B1051 Deployment Commanded | SDM | Yes
DTC B1053 Deployment Commanded w/Loop Malfunction | SDM | Yes
DTC B1061 Lamp Circuit Failure | SDM | Yes
DTC B1071 Internal SDM Failure | SDM | Yes