For 1990-2009 cars

When the system is powered up, the heater and A/C programmer initiates one or both of the following functions in order to avoid window fogging or other undesirable conditions:

• | Purge the system of stale air.

• | Redirect the air.

The programmer will determine if any undesirable conditions exist when the ignition is turned on or the heating, ventilation, and air conditioning (HVAC) system is in AUTO or VENT mode.

The programmer has the option of three different purge modes to select from to eliminate undesirable conditions.

### Normal Purge

Moisture tends to accumulate in the heating, ventilation, and air conditioning (HVAC) module after the engine has been shut off. When the engine is restarted and the A/C system turns on, the moisture may expel from the windshield or the instrument panel outlets. This causes window fogging.

On startup, the programmer inspects for indications that window fogging may occur. If window fogging is evident, the programmer initiates the following functions:

• | Delays the blower operation until the engine coolant temperature reaches 38°C (126°F).

• | Closes the defroster door.

• | Positions the A/C door in order to direct the air out the heater outlets.

• | Runs the blower at low speed.

The programmer then resumes normal system operation.

Operating the fan in MANUAL mode or selecting the MANUAL mode will bypass the normal purge mode.

### Cold Purge

In cold weather, moist breath air from the vehicle occupants may condense on the windshield.

On cold engine startup, the programmer inspects for indications that window fogging may occur. If window fogging is evident, the programmer initiates the following functions:

• | Positions the doors in order to direct air out the windshield outlets.

• | Operates the blower.

The programmer then resumes normal system operation.

Operating the fan in the MANUAL mode or selecting the MANUAL mode will bypass the cold purge mode.

### A/C Purge

Moisture tends to accumulate in the heating, ventilation, and air conditioning (HVAC) module after the engine has been shut off. Moisture may expel from the instrument panel outlets toward the front seat occupants when the engine is restarted or when the A/C is turned ON.

On the startup, the programmer inspects for indications of moisture. If moisture is evident, the programmer initiates the following functions:

• | Positions the A/C door in order to direct the air toward the floor.

• | Operates the blower.

The programmer then resumes the normal system operation.

Operating the fan in MANUAL mode or selecting any MANUAL mode will bypass the A/C purge mode.