For 1990-2009 cars

### Audible Warnings Operation

The audible warnings system informs the driver that one or more of the following conditions exist:

• | The exterior lights are on. Both of the following conditions are met:

- | The ignition switch is in any of the following positions:

• | LOCK

• | OFF

• | ACCY

- | The left front door is open.

• | The key is in the ignition. Both of the following conditions are met:

- | The ignition switch is in any of the following positions:

• | LOCK

• | OFF

• | ACCY

- | The left front door is open.

• | A safety belt is unbuckled. The ignition switch is in either of the following positions:

- | RUN

- | START

• | The vehicle has travelled over 1.2 km (3/4 mi) while a turn signal is on.

• | The vehicle has travelled approximately 12 m (40 ft) while the parking brake is engaged.

### Chime Priorities

When multiple chimes are required, only the chime with the highest priority sounds. The chimes are prioritized as follows:

1. The fasten seat belts warning chime overrides all other simultaneous audible chimes.
2. The key-in-ignition warning chime overrides the lamps on warning chime if both exist simultaneously.

### Chime Rates

The rates of chime operation are as follows:

• | The fasten belts warning chime rate is 50 pulses per minute.

• | The lamps on warning chime rate is 150 pulses per minutes.

• | The key-in-ignition warning chime rate is 200 pulses per minute.