For 1990-2009 cars

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---
1 |

1. Turn the ignition switch to RUN.
2. Depress the brake pedal.
3. Attempt to move the gear selector lever out of the PARK position.

The shift interlock feature prevents the gear selector lever from shifting out of PARK.

Automatic Transmission Shift Lock Control Inoperative

2 |

1. Turn the ignition switch to RUN.
2. Depress the brake pedal.
3. Attempt to move the gear shift lever out of the PARK position.

The gear selector lever shifts out of the PARK position.

Automatic Transmission Shift Lock Control Always On With Ignition in RUN

* Refer to the appropriate symptom diagnostic table for the applicable abnormal result.