For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Frame Insulator Bolt to Body | 192 N·m | 142 lb ft
Left Transaxle Mount-to-Frame | 65 N·m | 48 lb ft
Negative Battery Cable | 15 N·m | 11 lb ft
Power Steering Lines to Frame | 6 N·m | 53 lb in
Rack and Pinion Bolts | 65 N·m | 48 lb ft
Right Transaxle Mount-to-Bracket Bolt and Nut | 95 N·m | 70 lb ft
Wheel Nuts | 140 N·m | 100 lb ft