For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Radio/Audio System Check? | -- | Go to Step 2 | Go to Radio/Audio System Check
2 |

1. Disconnect the compact disc (CD) player.
2. Measure the voltage between the CD player connector terminal 5 and ground.

Is the voltage within the specified range?

10-15V

Go to Step 4

Go to Step 3

3 | Repair the open or short to ground in CKT 440 (ORN). Did you complete the repair? | -- | Go to Radio/Audio System Check | --
4 | Measure the voltage between the CD changer connector terminal 5 and 7. Is the voltage within the specified range? | 10-15V | Go to Step 5 | Go to Step 6
5 | Repair the open in CKT 1051 (BLK). Did you compete the repair? | -- | Refer to Radio/Audio System Check | --
6 | Inspect the CKT 835 (DK GRN) for an open or short to ground or power. Is CKT 835 open or shorted? | -- | Go to Step 7 | Go to Step 8
7 | Repair the open or short in CKT 835 (DK GRN). Did you complete the repair? | -- | Refer to Radio/Audio System Check | --
8 | Replace the CD changer. Refer to Remote CD Changer Replacement . Did you complete the repair? | -- | Refer to Radio/Audio System Check | --