For 1990-2009 cars

### Removal Procedure

1. Remove the air cleaner intake duct. Refer to Air Cleaner Inlet Duct Replacement in Engine Controls.
2. Drain the coolant from the surge tank. Refer to Cooling System Draining and Filling .
3. Disconnect the clamps and hoses .
4. Remove the fasteners retaining the reservoir.
5. Lift up the reservoir and disconnect the low coolant level sensor electrical connector.
6. Remove the surge tank.

### Installation Procedure

1. Connect the low coolant level sensor electrical connector.
2. Install the surge tank in position in the vehicle.
3. Install the fasteners.
4. Connect the hoses and clamps to the surge tank.
5. Refill the surge tank with coolant. Refer to Cooling System Draining and Filling .
6. Install the air cleaner intake duct. Refer to Air Cleaner Inlet Duct Replacement in Engine Controls.