For 1990-2009 cars

## Front Side Door Air Duct and Outlet Replacement Buick

### Removal Procedure

1. Remove the trim panel (3). Refer to Door Trim Panel Replacement .
2. Remove the 2 clips that retain the HVAC duct (1).
3. Remove the HVAC duct (1) and gasket (2).

### Installation Procedure

1. Install the HVAC duct (1) and gasket (2).
2. Install the 2 clips in order to retain the HVAC duct (1).
3. Install the trim panel (3). Refer to Door Trim Panel Replacement

## Front Side Door Air Duct and Outlet Replacement Oldsmobile

### Removal Procedure

1. Remove the trim panel (3). Refer to Front Side Door Trim Panel Replacement or Rear Side Door Trim Panel Replacement .
2. Remove the fasteners from the trim panel plate (10) and the armrest (11).
3. Remove the trim panel plate (10) and the armrest (11).
4. Remove the HVAC duct (9) from the gasket.

### Installation Procedure

1. Install the HVAC duct (9) into the gasket.
2. Install the trim panel plate (10).
3. Install the armrest (11).
4. Install the trim panel plate (10) fasteners.
5. Install the armrest (11) fasteners in order to retain the armrest to the panel.
6. Install the trim panel (3). Refer to Front Side Door Trim Panel Replacement or Rear Side Door Trim Panel Replacement .