For 1990-2009 cars

### Removal Procedure

1. Remove the lower pillar garnish molding (5).
2. Remove the shoulder belt guide bolt from the B-pillar. Refer to Seat Belt Replacement - Driver or Passenger in Seat Belts.
3. Remove the upper pillar garnish molding (3) in order to disengage the clips.

### Installation Procedure

1. Install the upper pillar garnish molding (3).
2. Push in the molding (3) in order to install the molding to the vehicle.
3. Install the shoulder belt bolt and guide. Refer to Seat Belt Replacement - Driver or Passenger in Seat Belts.
4. Install the lower pillar garnish molding (5).