For 1990-2009 cars

### Removal Procedure

1. Remove the left side sound insulator. Refer to Instrument Panel Insulator Panel Replacement - Left Side in Instrument Panel, Gauges and Console.
2. Disconnect the electrical connector.
3. Remove the theft deterrent relay (2).

### Installation Procedure

1. Install the theft deterrent relay (2).
2. Connect the electrical connector.
3. Install the sound insulator. Refer to Instrument Panel Insulator Panel Replacement - Left Side in Instrument Panel, Gauges and Console.