For 1990-2009 cars

The Remote Activation Verification (RAV) provides feedback to the driver that the vehicle has received as the command from the transmitter.

The driver may select the following modes:

Mode | Unlock Vehicle | Lock Vehicle
--- | --- | ---
0 | Turn the feature off |
1 | Single flash exterior lamps | No feedback
2 | No feedback | Single flash exterior lamps
3 | Single flash exterior lamps | Single flash exterior lamps
4 | No feedback | Single flash exterior lamps and chirp horn
5 | Single flash exterior lamps | Single flash exterior lamps and chirp horn

Customize the activation feature to each transmitter using the following procedure:

1. Hold the power door lock switch down.

The doors lock.

2. Press the TRUNK button on the transmitter.

The RAV mode stays in the current mode. The horn chirps.

3. Press the TRUNK button on the transmitter.

The RAV mode changes to the next mode. The horn chirps.

4. Release the power door lock switch.

The customization mode terminates.