For 1990-2009 cars

### Removal Procedure

1. Insert a flat bladed tool (1) at the rear edge of the universal garage door opener.
2. Disengage the forward tabs (2) from the overhead console.
3. Disconnect the electrical connector.
4. Remove the screws (1) from the universal garage door opener (2) to overhead console.

### Installation Procedure

1. Install the screws (1) that attach the universal garage door opener (2) to the roof console.
2. Connect the electrical connector to the garage door opener.
3. Position the access door and align the rear tabs into the overhead console.
4. Push upward in order to engage the front tab.