For 1990-2009 cars

## Front Side Door Window Module Replacement Express Down Module

### Removal Procedure

Caution: Disconnect the power window switch when working inside the driver door. When operated, the Express Up/Down Feature allows the door window to move very quickly, without stopping, which could cause personal injury.

1. Remove the door trim panel. Refer to Front Side Door Trim Panel Replacement .
2. Release the retaining clip securing the express down module to the door.
3. Disconnect the CPA retainer.
4. Disconnect the electrical connector.
5. Remove the express down module (1).

### Installation Procedure

1. Connect the electrical connector.
2. Install the CPA retainer.
3. Connect the express down module to the door with the retainer clip.
4. Install the door trim panel. Refer to Front Side Door Trim Panel Replacement .