For 1990-2009 cars

## Ignition and Key Alarm Switch Assembly - Disassemble - Off Vehicle Olds

### Disassembly Procedure

1. Remove the upper and lower covers. Refer to Steering Column Trim Covers - Disassemble - Off Vehicle .
2. Remove the connector from the ignition switch assembly.
3. Remove 2 tapping screws.
4. Remove the ignition switch assembly.

## Ignition and Key Alarm Switch Assembly - Disassemble - Off Vehicle Buick

### Disassembly Procedure

1. Remove the upper and lower covers. Refer to Steering Column Trim Covers - Disassemble - Off Vehicle .
2. Remove the connector from the ignition switch assembly.
3. Remove 2 tapping screws.
4. Remove the ignition switch assembly.