For 1990-2009 cars

# FRONT DOOR HINGE REPAIR CHECK LINK ROLLER

Front door hinges on above listed models, with the check link roller, may be repaired with part number 20497383 (Figure 2) using the following procedure:

1. Using a #29 (.1360) drill bit, drill a hole 10 mm (3/8") from the roller end of the hinge stop pin (Figure 1).

2. Thread drilled hole using a #8-32 tdp.

3. Discard stop pin (Item 1, Figure 2) included in parts package.

4. Using a hammer, install roller, bushing and pin into hinge stop pin (Items 2, 3 and 4, Figure 2).

5. Install an 8-32 hexagon set screw (part number 9426939 or equivalent) into tapped hole and tighten to retain roller pin. Apply Loctite thread sealer (part number 1052624 or equivalent) to set screw threads prior to installation.

6. Install check link spring using tool J-29849 or equivalent.

7. Lubricate roller and bushing with 30 weight engine oil.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.