For 1990-2009 cars

# SERVICE MANUAL UPDATE SEC. 6E3 REVISED PCM TROUBLE CODE 47

#### SUBJECT: SERVICE MANUAL UPDATE - SECTION 6E3 - REVISED PCM TROUBLE CODE 47

#### VEHICLES AFFECTED: 1992 "E" 3800 (VIN L)

The 1992 "E" car service manuals do not include PCM Code 47. This bulletin provides diagnostics for PCM Code 47, BCM - PCM data circuit problem. When diagnosing a Code 47, refer to this bulletin and "Computer System Diagnosis" (SECTION 8D) in the service manual. This bulletin also revises the PCM diagnostic Codes table on Page 6E3-A-16 (Olds)/Page 6E3-A-17 (Buick).

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.