For 1990-2009 cars

# POOR PERFORMANCE WIDE OPEN CARBURETOR METERING RODS

#### Models Affected: 1982 & 1983 Regals & Rivieras Equipped With 4.1L Engines Carburetor Numbers 17082267 & 17082268

A poor performance comment may be received from a customer when operating their vehicles at wide open throttle. It may be described as running out of fuel when actually the engine is running too rich.

A secondary metering rod package (Rods coded "DZ") has been released for service an these vehicles.

Part Number 17075268

Service Manual procedures for removal and installation should be followed.

Labor operation: T5064 Labor time: 0.4 Failure code: 92

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.