For 1990-2009 cars

#### Fastener Tightening Specifications

Application | Specification
--- | ---
Metric | English
Accumulator Cover Bolt/Screw -- M6 x 1.0 x 28 (Qty 11) | 12 N·m | 106 lb in
Automatic Transaxle Case Cover Bolt/Screw -- M6 x 1.0 x 30 (Qty 3) | 12 N·m | 106 lb in
Automatic Transaxle Case Cover Bolt/Screw (TORX® Special) -- M6 x 1.0 x 32 (Qty 1) | 12 N·m | 106 lb in
Automatic Transaxle Case Cover Bolt/Screw -- M6 x 1.0 x 40 (Qty 3) | 12 N·m | 106 lb in
Automatic Transaxle Case Cover Bolt/Screw -- M8 x 1.25 x 50 (Qty 3) | 25 N·m | 18 lb ft
Automatic Transaxle Case Extension Bolt/Screw -- M10 x 1.5 x 35 (Qty 4) | 36 N·m | 26 lb ft
Automatic Transaxle Oil Pump Bolt/Screw -- M6 x 1.0 x 85 (Qty 9) | 12 N·m | 106 lb in
Automatic Transaxle Oil Pump Bolt/Screw -- M6 x 1.0 x 95 (Qty 2) | 16 N·m | 11 lb ft
Automatic Transaxle Oil Pump Cover Bolt/Screw -- M6 x 1.0 x 20 (Qty 1) | 8 N·m | 70 lb in
Automatic Transaxle Oil Pressure Test Hole Plug -- 1/8 - 27 NPTF (Qty 1) | 12 N·m | 106 lb in
Case Side Cover Bolt/Screw (Flange) -- M8 x 1.25 x 25 (Qty 9) | 25 N·m | 18 lb ft
Case Side Cover Bolt/Screw (stud) -- M8 x 1.25 x 24 (Qty 4) | 25 N·m | 18 lb ft
Case Side Cover Bolt/Screw (TORX® Special) -- M8 x 1.25 x 21 (Qty 4) | 25 N·m | 18 lb ft
Control Valve Body Bolt/Screw -- M6 x 1.0 x 20 (Qty 2) | 8 N·m | 70 lb in
Control Valve Body Bolt/Screw -- M6 x 1.0 x 30 (Qty 1) | 12 N·m | 106 lb in
Control Valve Body Bolt/Screw -- M6 x 1.0 x 55 (Qty 3) | 12 N·m | 106 lb in
Control Valve Body Bolt/Screw -- M6 x 1.0 x 60 (Qty 3) | 12 N·m | 106 lb in
Control Valve Body Bolt/Screw -- M6 x 1.0 x 65 (Qty 3) | 12 N·m | 106 lb in
Control Valve Body Bolt/Screw -- M6 x 1.0 x 85 (Qty 1) | 12 N·m | 106 lb in
Control Valve Body Bolt/Screw -- M6 x 1.0 x 95 (Qty 1) | 16 N·m | 11 lb ft
Control Valve Body Bolt/Screw -- M8 x 1.25 x 90 (Qty 1) | 25 N·m | 18 lb ft
Control Valve Body Bolt/Screw (TORX®) -- M6 x 1.0 x 45 (Qty 2) | 12 N·m | 106 lb in
Drive Sprocket Support Bolt/Screw -- M8 x 1.25 x 24 (Qty 4) | 25 N·m | 18 lb ft
Forward Band Servo Cover Bolt/Screw -- M6 x 1.0 x 20 (Qty 3) | 12 N·m | 106 lb in
Manual 2-1 Band Servo Cover Bolt/Screw -- M8 x 1.25 x 25 (Qty 3) | 25 N·m | 18 lb ft
Manual Shift Shaft Detent Bolt/Screw -- M6 x 1.0 x 16 (Qty 1) | 12 N·m | 106 lb in
Manual Shift Shaft Detent Lever Nut -- M10 x 1.5 (Qty 1) | 32 N·m | 23 lb ft
Oil Pan Bolt -- M6 x 1.0 x 17 (Qty 20) | 14 N·m | 10 lb ft
Transaxle Oil Cooler Pipe Fitting -- 1/4 - 18 NPSF (Qty 2) | 38 N·m | 28 lb ft
Vehicle Speed Sensor Stud/Screw -- M8 x 1.25 x 12 (Qty 1) | 12 N·m | 106 lb in