For 1990-2009 cars

### Removal Procedure

Important: The outer belt sealing strip/reveal moldings (1) are retained in the same manner for the front and the rear door. Both of the moldings have the following components:

• | Single stage clips that retain the moldings to the door belt

• | Locator pins in order to ensure proper positioning

The only difference between the front door and the rear door is the starting point for removal:

• | The starting point for the front door is at the rear.

• | The starting point for the rear door is at the front.

1. Lower the window to the full down position.

Important: If you use a metal tool, pad the tool with tape in order to protect the painted metal surface.

2. Use a flat thin-bladed tool in order to gently pry the molding (1) while rotating the molding outboard.

### Installation Procedure

1. Position the rear end of the molding (1) flush to the rear edge of the door.

Important: If the edge of the molding is not flush to the edge of the door, gently tap the molding into place, with a rubber mallet.

2. Slowly working forward with a rubber mallet, gently tap the molding into place.

Do NOT allow the close-out lip to roll under.

3. Ensure the sealing strip is securely retained onto the doors inner pinch-weld flange.