For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Interior Lamps System Check? | -- | Go to Step 2 | Go to Interior Lamps System Check
2 | Test for an open in CKT 32 (YEL) between S206 and the underhood lamp. Refer to Testing for Continuity in Wiring Systems. Is CKT 32 OK? | -- | Go to Step 3 | Go to Step 5
3 | Test for an open in CKT 1350 (BLK) between S115 and the underhood lamp. Refer to Testing for Continuity in Wiring Systems. Is CKT 1350 OK? | -- | Go to Step 4 | Go to Step 5
4 | Replace the underhood lamp. Refer to Underhood Lamp Replacement . Is the repair complete? | -- | Go to Interior Lamps System Check | --
5 | Repair the suspect wiring. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Interior Lamps System Check | --