For 1990-2009 cars

# SMU - SECTION 3A - REVISED ALIGNMENT SPECIFICATIONS

#### SUBJECT: SERVICE MANUAL UPDATE - SECTION 3A - REVISED ALIGNMENT SPECIFICATIONS FOR CAMBER ADJUSTMENT

#### MODELS: 1997 BUICK RIVIERA 1997 OLDSMOBILE AURORA

THIS BULLETIN IS BEING ISSUED TO REVISE THE ALIGNMENT SPECIFICATIONS FOR CAMBER ADJUSTMENT IN SECTION 3A OF THE SERVICE MANUAL.

THE FRONT CAMBER IS CURRENTLY LISTED AT +0.2 +/- 0.5 DEGREES. THE CORRECT CAMBER SPECIFICATION IS -0.2 +/- 0.5 DEGREES.

PLEASE UPDATE THE SERVICE MANUAL WITH THE REVISED CAMBER SPECIFICATIONS.

FIGURES: 00 ATTACHMENTS: 00

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1996 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.