For 1990-2009 cars

# APPLY RING & WAVE CLUTCH PLATE LO & REVERSE CLUTCH ASSEMBLY

BEGINNING OCTOBER, 1980, A NEW WAVED CLUTCH PLATE AND REDESIGNED APPLY RING IS IN PRODUCTION FOR ALL MODELS OF THE THM 325, 200, 200C, AND 200-4R TRANSMISSIONS. THE NEW DESIGN LO & REVERSE CLUTCH ASSEMBLY CONTAINS A WAVED CLUTCH PLATE AND THE APPLY RING WIDTH IS REDUCED TO ALLOW CLEARANCE FOR THIS EXTRA CLUTCH PLATE. SEE FIGURE 1. THE PAST DESIGN LO & REVERSE CLUTCH ASSEMBLY, WITHOUT THE WAVED CLUTCH PLATE, IS STILL AVAILABLE FOR SERVICE AS EXPLAINED BELOW. SEE FIGURE 2. ** CHARTS AND ILLUSTRATIONS IN BULLETIN **

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.