For 1990-2009 cars

#### Tools Required

J 7872 Magnetic Base Indicator Set

Important: The camshaft and lifters become mated to each other through both normal and premature wear. If the camshaft must be replaced, ALL lifters must be replaced as well.

1. Measure the camshaft journals with a micrometer.

If the camshaft journals are not within specifications, replace the camshaft. The measurement should be 47.655-46.858 mm (1.8462-1.8448 in). If the measurement is not within specifications the engine camshaft must be replaced.

2. Measure the camshaft runout using J 7872 .

2.1. | Mount the camshaft in V-blocks between centers.

2.2. | Use J 7872 to check the intermediate camshaft journal.

3. If the runout exceeds specifications, the camshaft is bent and should be replaced. If the camshaft journals are more than 0.025 mm (0.0010 in) out-of-round, then replace the engine camshaft.