For 1990-2009 cars

## Rear Compartment Lid Valet Lock Out Switch Replacement Buick

### Removal Procedure

1. Open the instrument panel storage compartment.
2. Carefully pry outward on the valet switch (1).
3. Disconnect the electrical connector (2).
4. Remove the valet switch (1).

### Installation Procedure

1. Connect the electrical connector to the valet switch (1).
2. Align the valet switch (1) to the instrument panel storage compartment.
3. Apply light downward pressure in order to fasten the switch.
4. Close the instrument panel storage compartment.

## Rear Compartment Lid Valet Lock Out Switch Replacement Oldsmobile

### Removal Procedure

1. Open the instrument panel storage compartment.
2. Carefully pry outward on the valet switch (1).
3. Disconnect the electrical connector (2).
4. Remove the valet switch (1).

### Installation Procedure

1. Connect the electrical connector (2) to the valet switch (1).
2. Install the valet switch (1) to the instrument panel storage compartment.
3. Apply light downward pressure in order to seat the switch.
4. Close the instrument panel storage compartment.