For 1990-2009 cars

### Removal Procedure

1. Remove the I/P assembly.
2. Disconnect the electrical connectors from the switches.
3. Remove the pushrod (2) from the pushrod pin (1).
4. Remove the six brake pedal nuts (1).
5. Remove the brake pedal assembly (1).

### Installation Procedure

1. Install the brake pedal assembly (1) onto the booster studs.
2. Install the six brake pedal nuts (1).
3. Apply the lubricant to the pushrod pin (1).

Use GM P/N 9985164 or the equivalent.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Install the pushrod (2) onto the pushrod pin (1). Secure with a spacer (3) and a retainer (4).

Tighten

• | Tighten the pedal assembly to the lower Cowl Stud Nuts to 16 N·m (12 lb ft).

• | Tighten the Pedal Assembly to the Booster Stud Nuts to 32 N·m (24 lb ft).

5. Connect the electrical connectors to the switches.
6. Install the I/P assembly.