For 1990-2009 cars

### Removal Procedure

1. Position the manual release cable through the slot in the rear compartment trim from the inside of the rear compartment.
2. Remove the push-in retainers (3) from the fuel filler door actuator (4).
3. Remove the fuel filler door actuator (4).
4. Disconnect the electrical connector (1) from the actuator (4).

### Installation Procedure

1. Connect the electrical connector (1) to the actuator (4).
2. Install the fuel filler door actuator (4).
3. Install the push-in retainers (3) to the fuel filler door actuator (4).
4. Insert the manual release cable (2) through the slot in the rear compartment trim.
5. Verify proper operation of the fuel filler door.