For 1990-2009 cars

#### Tools Required

J 36850 Transjel™

1. Inspect the thrust bearings (671, 674, 676) for the following:

• | A damaged cage

• | Damaged or missing rollers

2. Inspect the reaction carrier assembly (675) for damage to the pinion/internal gear teeth.
3. Inspect the input carrier assembly (672) for damage to the pinion/spline teeth.
4. Inspect the lube dam (673) for the following:

• | Cracks

• | Damage

5. Affix the thrust bearing (676) onto the reaction carrier (675). Use J 36850 or equivalent in order to retain the bearing.
6. Install the reaction carrier (675) into the case and rotate the carrier so that the pinions engage the reaction sun gear.
7. Affix the thrust bearing (674) into the input carrier (675). Use J 36850 or equivalent in order to retain the bearing.
8. Install the lube dam (673) into the reaction carrier assembly (675). Use J 36850 or equivalent in order to retain the dam.
9. Insert the input carrier assembly (672) into the case and rotate the carrier so that the pinions engage the reaction carrier internal gear.