For 1990-2009 cars

### Removal Procedure

1. Remove the resistor bolt (2) from the left front fender.
2. Disconnect the connector (1).
3. Remove the daytime running lamp resistor (3).

### Installation Procedure

1. Connect the connector (1) to the daytime running lamp resistor (3).
2. Install the daytime running lamp resistor (3) to the front fender.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the resistor bolt (2) to the front fender.

Tighten
Tighten the bolt to 7 N·m (62 lb in).