For 1990-2009 cars

# DOOR CREAK NOISE AND OR DOOR FRAME PAINT MARRED

DOOR CREAK NOISE AND/OR INNER DOOR FRAME PAINT MARRED

#### VEHICLES AFFECTED: 1986-1987 ELDORADO AND SEVILLE ------------------ Some Eldorados and Sevilles may exhibit a condition of a creaking or popping noise at the "A" pillar area. There may also be evidence of paint being marred on the inner door frame in the radius area (see Figure 1) or down the "A" pillar. Sevilles can also exhibit this paint marring on the rear doors where the roof meets the sail panel.

The noise and marring may be caused by the roof drip flange cover contacting the inner door frame at the points where the paint is marred.

To repair this condition, perform the following:

1. Remove roof drip flange cover and inspect. Remove any excessive thumbgrade sealer and/or black sealing tape from area shown in Figure 1.

#### NOTE: Only one layer of black sealing tape is required, excess sealing tape is usually folded over on the roof drip flange.

2. Using vise grips, bend corner of roof drip flange up 1/2" as shown in Figure 1.

3. Install roof drip flange cover and use sheet metal screws with flat washers instead of screws with countersink heads in the three hole locations on the "A" Pillar.

4. Hand start the "A" Pillar attaching screws.

5. Lift the roof drip flange cover up in direction shown in Figure 1 for clearance between the roof drip flange cover and inner door frame. It may be necessary to enlarge the three "A" Pillar attaching holes in the drip flange for the necessary adjustment.

6. Tighten the "A" Pillar attaching screws.

7. Drill hole for sheet metal screw in radius of roof drip flange cover, see Figure 1. Install sheet metal screw and flat washer to roof drip flange cover.

8. For Seville, repeat step 7 at rear radius of roof drip flange cover, see Figure 1.

Use the most applicable labour operation from the Canadian Labour Time Guide and claim the applicable time:

Front Doors .5 hours Rear Doors .2 hours

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.