For 1990-2009 cars

### Removal Procedure

1. Remove the fuel injector sight shield if necessary. Refer to Fuel Injector Sight Shield Replacement in Engine Mechanical.
2. Disconnect the cruise control cable from the following locations:

• | The engine bracket

• | The TBI cam

3. Disconnect the cruise control cable (2) from the module assembly (1).
4. Disconnect the electrical connector from the module assembly (1).
5. Remove the 2 fasteners (1) from the mounting studs.
6. Remove the module assembly (2).
7. Remove the fasteners (4) retaining the module to the mounting bracket.

### Installation Procedure

1. Install the module to the mounting bracket.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the module fasteners (4).

Tighten
Tighten the fasteners to 6.5 N·m (57 lb in).

3. Install the module assembly (2) onto the mounting studs.
4. Install the 2 fasteners (1) to the mounting studs.

Tighten
Tighten the nuts to 9 N·m (80 lb in).

5. Connect the electrical connector to the module assembly (2).
6. Connect the cruise control cable (2) to the following locations:

• | The module assembly

• | The engine bracket

• | The TBI cam

7. Adjust the cable. Refer to Cruise Control Cable Adjustment .
8. Install the fuel injector sight shield if necessary. Refer to Fuel Injector Sight Shield Replacement in Engine Mechanical.