For 1990-2009 cars

### Removal Procedure

1. Remove the seat assembly. Refer to Seat Replacement .
2. Remove the fasteners that retain the memory module (1) to the seat assembly.
3. Disconnect the electrical connectors.
4. Remove the memory module (1).

### Installation Procedure

1. Install the memory module (1).
2. Connect the electrical connectors.
3. Install the fasteners in order to retain the memory module to the seat assembly.
4. Install the seat assembly. Refer to Seat Replacement .
5. Calibrate the seat. Refer to Memory Seat Calibration .