For 1990-2009 cars

### Removal Procedure

1. Remove the hood latch assembly. Refer to Hood Primary and Secondary Latch Replacement .
2. Remove the bolts (3) retaining the hood latch support (2).
3. Remove the hood latch support (2).

### Installation Procedure

1. Install the hood latch support (2).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the bolts (3).

Tighten
Tighten the bolts to 10.5 N·m (93 lb in).

3. Install the hood primary latch assembly. Refer to Hood Primary and Secondary Latch Replacement .
4. Adjust the latch as needed.