For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Instrument Cluster System Check? | -- | Go to Step 2 | Go to Diagnostic System Check - Instrument Cluster
2 |

1. Disconnect the windshield washer solvent level switch connector.
2. Turn the ignition switch to the RUN position.
3. Measure the voltage between connector terminal B (BLK) and ground.

Does the measured voltage equal the specified value?

12 V

Go to Step 5

Go to Step 3

3 | Inspect CKT 99 (BLK) for a open or short to ground. Is the wiring OK? | -- | Go to Step 6 | Go to Step 4
4 | Repair the wiring in CKT 99 (BLK). Is the repair complete? | -- | Go to Instrument Cluster System Check | --
5 | Measure the voltage between the connector terminal B (BLK) and the connector terminal A (BLK). Does the measured voltage equal the specified value? | 12 V | Go to Step 11 | Go to Step 8
6 | Inspect the instrument cluster connector C1 for proper terminal contact. Is the terminal OK? | -- | Go to Step 15 | Go to Step 14
7 | Replace the instrument cluster. Is the repair complete? | -- | Go to Instrument Cluster System Check | --
8 | Inspect CKT 1350 (BLK) for a open Is the wiring OK? | -- | Go to Step 10 | Go to Step 9
9 | Repair the wiring in CKT 1350 (BLK). Is the repair complete? | -- | Go to Step 10 | --
10 | Inspect the in-line connector C105 for proper terminal contact. Is the terminal OK? | -- | Go to Instrument Cluster System Check | --
11 | Inspect the windshield washer solvent level switch connector for proper terminal contact. Is the terminal OK? | -- | Go to Step 12 | Go to Step 13
12 | Replace the washer fluid level switch. Is the repair complete? | -- | Go to Instrument Cluster System Check | --
13 | Repair the windshield washer solvent level switch connector terminals. Is the repair complete? | -- | Go to Instrument Cluster System Check | --
14 | Repair the poor connection. Is the repair complete? | -- | Go to Instrument Cluster System Check | --
15 | Inspect the in-line connector C105 for proper terminal contact. Are the terminals OK? | -- | Go to Step 7 | Go to Step 14