For 1990-2009 cars

Important: The steering column must be in the 12 o'clock position.

1. Align the block tooth on the race and upper shaft assembly in the 12 o'clock position.
2. Install the wave washer (3).
3. Install the SIR coil assembly (2).
4. Install the retaining ring (1).
5. Install the SIR coil assembly connector to the fused jumper assembly connector.
6. Connect the wire harness assembly to the wire harness strap (1).
7. Install the upper cover and the lower cover. Refer to Steering Column Trim Covers - Assemble - Off Vehicle .