For 1990-2009 cars

# DELAYED 2-3 SHIFT THM 325 INTERMEDIATE BAND APPLY PIN

THM 325 2-3 DELAYED SHIFT A DELAYED 2-3 SHIFT ON THM 325 AUTOMATIC TRANSMISSIONS MAY BE CAUSED BY AN IMPROPERLY SIZED INTERMEDIATE BAND APPLY PIN. REFER TO THE 1981 SERVICE MANUAL (FIGURE 7B-37, INTERMEDIATE BAND APPLY PIN SELECTION CHART) FOR CORRECT PIN USAGE. DIMENSION FOR 2-RING APPLY PIN SHOULD BE AS FOLLOWS: .72MM-1.44MM (.029"-.057").

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.