Brake Transmission Shift Interlock Solenoid Replacement. Buick Roadmaster 1996

For 1990-2009 cars

### Removal Procedure

Important: For Brake Transmission Shift Interlock Solenoid (BTSI) removal and installation procedures with column shift, refer to Steering Column Unit Repair.

1. Remove the shifter handle and the retainer.
2. Remove the floor console trim plate. Refer to Front Floor Console in Instrument Panel and Gauges.
3. Disconnect the BTSI solenoid electrical connector.
4. Remove the BTSI solenoid (869) and the attaching clips.

### Installation Procedure

Important: For Brake Transmission Shift Interlock Solenoid (BTSI) removal and installation procedures with column shift, refer to Steering Column Unit Repair.

1. Install the BTSI solenoid and the attaching clips.
2. Connect the BTSI solenoid electrical connector.
3. Install the floor console trim plate. Refer to Front Floor Console in Instrument Panel and Gauges.
4. Install the shifter handle and the retainer.