Battery Usage. Buick Roadmaster 1996

For 1990-2009 cars

Application | Description
--- | ---
Catalog Number | 514
Cold Cranking Amperage (CCA) | 525
Load Test (AMPS) | 260
Replacement Model Number | 75-60
Reserve Capacity Minutes | 90
Catalog Number | 744
Cold Cranking Amperage (CCA) | 770
Load Test (AMPS) | 380
Replacement Model Number | 78A-72
Reserve Capacity Minutes | 115
Catalog Number | 746
Cold Cranking Amperage (CCA) | 770
Load Test (AMPS) | 380
Replacement Model Number | 78A-72
Reserve Capacity Minutes | 115