1-2 Accumulator Assemble. Buick Roadmaster 1996

For 1990-2009 cars

### Installation Procedure

1. Inspect the 1-2 accumulator piston for the following defects:

• | Porosity

• | Cracks

• | Scoring

• | Nicks and Scratches

2. Install a 1-2 accumulator piston seal on the 1-2 accumulator piston.
3. Inspect the 1-2 accumulator housing for the following defects:

• | Porosity

• | Cracks

• | Scoring

• | Nicks and Scratches

4. Install the 1-2 inner and outer accumulator springs.
5. Install the 1-2 accumulator piston.